**Greg’s Notes**

1. SPI1 (IMU) SCK set to 10 MHz. Datasheets says max is 20 MHz.